OUT

GND

+5V